Connecting Rpi to windows through SSH

1.Go to RPi. Run below command

Sudo Raspi-Config

Go to SSH settings in advance and enable it.

2. check inet address of Ethernet cable (if connecting through Ethernet)-> note this IP address.

3. In windows machine, install putty.

5. Put the IP we noted above and connect.

6. Use username as ‘pi’ and password as ‘raspberry’.

We are connected.